(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "User" 159.995 150.012)
  (title_block
    (title "Digi-Roll")
    (date "2024-09-04")
    (rev "1")
    (company "zbauman3")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "Net-(D1-K)")
  (net 4 "Net-(D1-A)")
  (net 5 "Net-(D2-K)")
  (net 6 "Net-(D2-A)")
  (net 7 "Net-(D3-K)")
  (net 8 "Net-(D3-A)")
  (net 9 "Net-(D4-K)")
  (net 10 "Net-(D4-A)")
  (net 11 "Net-(D5-K)")
  (net 12 "Net-(D5-A)")
  (net 13 "Net-(D6-K)")
  (net 14 "Net-(D6-A)")
  (net 15 "Net-(D7-K)")
  (net 16 "Net-(D7-A)")
  (net 17 "Net-(U1-XTAL1{slash}PB0)")
  (net 18 "Net-(U1-XTAL2{slash}PB1)")
  (net 19 "Net-(J1-MISO)")
  (net 20 "Net-(U1-PB2)")
  (net 21 "Net-(U1-PA7)")
  (net 22 "Net-(J1-SCK)")
  (net 23 "Net-(J1-MOSI)")
  (net 24 "Net-(J1-~{RST})")
  (net 25 "Net-(U1-PA3)")
  (net 26 "Net-(U1-PA2)")
  (net 27 "Net-(U1-PA1)")
  (net 28 "Net-(U1-AREF{slash}PA0)")
  (net 29 "unconnected-(U2-QH-Pad7)")
  (net 30 "unconnected-(U2-QH'-Pad9)")
  (net 31 "unconnected-(U3-GS-Pad14)")
  (net 32 "unconnected-(U6-EN-Pad4)")
  (net 33 "Net-(BT1-+)")
  (net 34 "Net-(U3-D7)")
  (net 35 "Net-(U3-D6)")
  (net 36 "Net-(U3-D5)")
  (net 37 "Net-(U3-D4)")
  (net 38 "Net-(U3-D3)")
  (net 39 "Net-(U3-D2)")
  (net 40 "Net-(U3-D1)")
  (net 41 "Net-(U3-D0)")
  (net 42 "Net-(J1-VCC)")
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 71.856664 92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "2.4K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D4-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Zane:Adafruit_7_seg" (layer "F.Cu")
    (at 49 35.094999)
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Adafruit 0.56\" 4-Digit 7-Segment Display w/ I2C Backpack - STEMMA QT / qwiic")
    (property "ki_keywords" "Adafruit 4-Digit 7-Segment LED I2C Backpack")
    (attr through_hole)
    (fp_text reference "U4" (at -16.854252 13.427107 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at -0.004121 13.712702 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 15.322833 13.427107 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.905001 -9.524999 270) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.1016))
    (pad "26" thru_hole circle (at 3.174999 -9.524999 270) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(J1-SCK)") (pinfunction "SCL") (pintype "input") (solder_mask_margin 0.1016))
    (pad "27" thru_hole circle (at 0.634999 -9.524999 270) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(J1-MOSI)") (pinfunction "SDA") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "28" thru_hole circle (at -4.445001 -9.524999 270) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.1016))
  )
  (footprint "Package_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (at 21.84 62.62 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "8-bit serial in/out Shift Register 3-State Outputs")
    (property "ki_keywords" "HCMOS SR 3State")
    (attr through_hole)
    (fp_text reference "U2" (at 3.82184 8.881657 90) (layer "F.SilkS"))
    (fp_text value "74HC595" (at 4.62 15.16 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D2-A)") (pinfunction "QB") (pintype "tri_state"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D3-A)") (pinfunction "QC") (pintype "tri_state"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-A)") (pinfunction "QD") (pintype "tri_state"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D5-A)") (pinfunction "QE") (pintype "tri_state"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D6-A)") (pinfunction "QF") (pintype "tri_state"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D7-A)") (pinfunction "QG") (pintype "tri_state"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(U2-QH-Pad7)") (pinfunction "QH") (pintype "tri_state"))
    (pad "8" thru_hole rect (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(U2-QH'-Pad9)") (pinfunction "QH'") (pintype "output"))
    (pad "10" thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "~{SRCLR}") (pintype "input"))
    (pad "11" thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(U1-AREF{slash}PA0)") (pinfunction "SRCLK") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(U1-PA2)") (pinfunction "RCLK") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "~{OE}") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U1-PA1)") (pinfunction "SER") (pintype "input"))
    (pad "15" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "QA") (pintype "tri_state"))
    (pad "16" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 96.725 86)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D6" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D6-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D6-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 118.725 79)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D7" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D7-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D7-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 94.19 96)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R13" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(U3-D2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 91.63 61.5 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole rect (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 63.224998 72)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D3" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D3-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 38.356666 96)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(U3-D7)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 34.81 96 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R15" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(U3-D0)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 85.55833 72)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D5" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D5-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D5-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 52.058332 86)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D2" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 83.02333 92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "2.4K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D5-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 94.19 92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "2.4K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D6-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (at 62.249998 87 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW3" (at 3.24899 2.27419 270) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(U3-D5)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (at 117.75 63.5 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW7" (at 3.268723 2.25 270) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(U3-D1)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (at 95.749996 77.5 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW6" (at 3.276411 2.252778 270) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(U3-D2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(U3-D2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 66.875 61.5 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 2.527471 -0.02653 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (at 84.58333 87 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW5" (at 3.254338 2.248807 270) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(U3-D3)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 74.391664 86)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D4" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (at 39.916666 87 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.255063 2.273623 270) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(U3-D7)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (at 73.416664 77.5 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW4" (at 3.263597 2.244703 90) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(U3-D4)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 84.447799 34.475)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch, separate symbol")
    (property "ki_keywords" "switch lever")
    (attr through_hole)
    (fp_text reference "SW9" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "SW_DPST_x2" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(BT1-+)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(J1-VCC)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 40.891666 72)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D1" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 116.19 92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "2.4K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D7-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (at 28.75 77.5 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW8" (at 3.242211 2.249999 270) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(U3-D0)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 71.856664 96)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R11" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(U3-D4)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 49.523332 92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "2.4K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D2-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (at 63 55 -90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "CMOS 8-Bit Priority Encoder")
    (property "ki_keywords" "8-Bit Priority Encoder")
    (attr through_hole)
    (fp_text reference "U3" (at 3.794715 8.907128 90) (layer "F.SilkS"))
    (fp_text value "~" (at 5.62 14) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(U3-D4)") (pinfunction "D4") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(U3-D5)") (pinfunction "D5") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(U3-D6)") (pinfunction "D6") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(U3-D7)") (pinfunction "D7") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "EI") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U1-PB2)") (pinfunction "Q2") (pintype "output"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(U1-XTAL2{slash}PB1)") (pinfunction "Q1") (pintype "output"))
    (pad "8" thru_hole rect (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "9" thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J1-MISO)") (pinfunction "Q0") (pintype "output"))
    (pad "10" thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(U3-D0)") (pinfunction "D0") (pintype "input"))
    (pad "11" thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(U3-D1)") (pinfunction "D1") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(U3-D2)") (pinfunction "D2") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(U3-D3)") (pinfunction "D3") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(U3-GS-Pad14)") (pinfunction "GS") (pintype "output"))
    (pad "15" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U1-PA7)") (pinfunction "EO") (pintype "output"))
    (pad "16" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Zane:Adafruit_Miniboost" (layer "F.Cu")
    (at 98 55.92)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Adafruit MiniBoost 5V @ 1A - TPS61023")
    (property "ki_keywords" "Adafruit MiniBoost 5V TPS61023")
    (attr through_hole)
    (fp_text reference "U6" (at 15.066133 -0.730128 90) (layer "F.SilkS"))
    (fp_text value "~" (at 8.328341 8.492888) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 1.905 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(J1-VCC)") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" thru_hole rect (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "5V") (pintype "power_out"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(U6-EN-Pad4)") (pinfunction "EN") (pintype "input"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 60.689998 92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "2.4K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D3-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 116.19 96)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R14" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(U3-D1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 83.02333 96)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R12" (at 3.746585 0.003594) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(U3-D3)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 97 34.475)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Hall Effect Sensor Switch")
    (property "ki_keywords" "Hall Effect Sensor Switch")
    (attr through_hole)
    (fp_text reference "U5" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "~" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U1-PA3)") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" thru_hole rect (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(U1-XTAL1{slash}PB0)") (pinfunction "OUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (at 51.083332 77.5 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW2" (at 3.25138 2.241841 270) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(U3-D6)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 49.523332 96)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R9" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(U3-D6)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 38.356666 92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "2.4K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (at 71 62.62 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-14")
    (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 7.7 90) (layer "F.SilkS"))
    (fp_text value "ATtiny84-20P" (at 5.62 13 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(U1-XTAL1{slash}PB0)") (pinfunction "XTAL1/PB0") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(U1-XTAL2{slash}PB1)") (pinfunction "XTAL2/PB1") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(J1-~{RST})") (pinfunction "~{RESET}/PB3") (pintype "bidirectional"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U1-PB2)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U1-PA7)") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(J1-MOSI)") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J1-MISO)") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(J1-SCK)") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "10" thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U1-PA3)") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(U1-PA2)") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U1-PA1)") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(U1-AREF{slash}PA0)") (pinfunction "AREF/PA0") (pintype "bidirectional"))
    (pad "14" thru_hole rect (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 60.689998 96)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(U3-D5)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 132.258299 57.92 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Atmel 6-pin ISP connector")
    (property "ki_keywords" "AVR ISP Connector")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 2.33) (layer "B.SilkS"))
    (fp_text value "AVR-ISP-6" (at 1.27 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J1-MISO)") (pinfunction "MISO") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(J1-VCC)") (pinfunction "VCC") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(J1-SCK)") (pinfunction "SCK") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(J1-MOSI)") (pinfunction "MOSI") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(J1-~{RST})") (pinfunction "~{RST}") (pintype "passive"))
    (pad "6" thru_hole rect (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "B.Cu")
    (at 90 51 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "digi-roll.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Multiple-cell battery")
    (property "ki_keywords" "batt voltage-source cell")
    (attr through_hole)
    (fp_text reference "BT1" (at 0 2.33 90) (layer "B.SilkS"))
    (fp_text value "Battery" (at 0 -4.87 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.27) (layer "B.Fab"))
    (pad "1" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(BT1-+)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole rect (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 23 23) (end 24.1 23)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 19 19) (end 108 19)
    (layer "Edge.Cuts"))
  (gr_line (start 139 99) (end 19 99)
    (layer "Edge.Cuts"))
  (gr_circle (center 23 95) (end 24.1 95)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 122 50) (end 139 50)
    (layer "Edge.Cuts"))
  (gr_line (start 108 36) (end 108 19)
    (layer "Edge.Cuts"))
  (gr_line (start 139 50) (end 139 99)
    (layer "Edge.Cuts"))
  (gr_circle (center 104 23) (end 105.1 23)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 19 99) (end 19 19)
    (layer "Edge.Cuts"))
  (gr_circle (center 135 95) (end 136.1 95)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 122 50) (mid 112.100506 45.899495) (end 108 36)
    (layer "Edge.Cuts"))
  (gr_text "5V" (at 127.785489 58.49919) (layer "B.SilkS"))
  (gr_text "GND" (at 128.032605 63.738061) (layer "B.SilkS"))
  (dimension (type aligned) (layer "User.1")
    (pts (xy 18.999999 19) (xy 18.999999 99))
    (height 1.999999)
    (gr_text "80.0000 mm" (at 15.85 59 90) (layer "User.1"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 18.999999 99) (xy 138.999999 99))
    (height 3)
    (gr_text "120.0000 mm" (at 78.999999 100.85) (layer "User.1"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 23.999999 79) (xy 23.999999 93))
    (height 2)
    (gr_text "14.0000 mm" (at 20.849999 86 90) (layer "User.1"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 133.999999 65) (xy 133.999999 93))
    (height -3)
    (gr_text "28.0000 mm" (at 135.849999 79 90) (layer "User.1"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
)
