(kicad_sch (version 20230121) (generator eeschema)
  (paper "User" 210.007 210.007)
  (title_block
    (title "Digi-Roll")
    (date "2024-08-22")
    (rev "1")
    (company "zbauman3")
  )
  (lib_symbols
    (symbol "4xxx:4532" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 5.08 11.43 0))
      (property "Value" "" (at 2.54 -2.54 0))
      (property "Footprint" "" (at 2.54 -2.54 0))
      (property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4532b.pdf" (at 2.54 -2.54 0))
      (property "ki_keywords" "8-Bit Priority Encoder" (at 0 0 0))
      (property "ki_description" "CMOS 8-Bit Priority Encoder" (at 0 0 0))
      (symbol "4532_1_1"
        (rectangle (start -6.35 10.16) (end 6.35 -10.16)
          (fill (type background))
        )
        (text "4532" (at 5.08 -11.43 0))
        (pin input line (at 8.89 1.27 180) (length 2.54)
          (name "D4")
          (number "1")
        )
        (pin input line (at 8.89 -8.89 180) (length 2.54)
          (name "D0")
          (number "10")
        )
        (pin input line (at 8.89 -6.35 180) (length 2.54)
          (name "D1")
          (number "11")
        )
        (pin input line (at 8.89 -3.81 180) (length 2.54)
          (name "D2")
          (number "12")
        )
        (pin input line (at 8.89 -1.27 180) (length 2.54)
          (name "D3")
          (number "13")
        )
        (pin output line (at -8.89 -6.35 0) (length 2.54)
          (name "GS")
          (number "14")
        )
        (pin output line (at -8.89 -8.89 0) (length 2.54)
          (name "EO")
          (number "15")
        )
        (pin power_in line (at 0 12.7 270) (length 2.54)
          (name "VDD")
          (number "16")
        )
        (pin input line (at 8.89 3.81 180) (length 2.54)
          (name "D5")
          (number "2")
        )
        (pin input line (at 8.89 6.35 180) (length 2.54)
          (name "D6")
          (number "3")
        )
        (pin input line (at 8.89 8.89 180) (length 2.54)
          (name "D7")
          (number "4")
        )
        (pin input line (at -8.89 -1.27 0) (length 2.54)
          (name "EI")
          (number "5")
        )
        (pin output line (at -8.89 8.89 0) (length 2.54)
          (name "Q2")
          (number "6")
        )
        (pin output line (at -8.89 6.35 0) (length 2.54)
          (name "Q1")
          (number "7")
        )
        (pin power_in line (at 0 -12.7 90) (length 2.54)
          (name "VSS")
          (number "8")
        )
        (pin output line (at -8.89 3.81 0) (length 2.54)
          (name "Q0")
          (number "9")
        )
      )
    )
    (symbol "74xx:74HC595" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -7.62 13.97 0))
      (property "Value" "74HC595" (at -7.62 -16.51 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc595.pdf" (at 0 0 0))
      (property "ki_keywords" "HCMOS SR 3State" (at 0 0 0))
      (property "ki_description" "8-bit serial in/out Shift Register 3-State Outputs" (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*" (at 0 0 0))
      (symbol "74HC595_1_0"
        (pin tri_state line (at 10.16 7.62 180) (length 2.54)
          (name "QB")
          (number "1")
        )
        (pin input line (at -10.16 2.54 0) (length 2.54)
          (name "~{SRCLR}")
          (number "10")
        )
        (pin input line (at -10.16 5.08 0) (length 2.54)
          (name "SRCLK")
          (number "11")
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "RCLK")
          (number "12")
        )
        (pin input line (at -10.16 -5.08 0) (length 2.54)
          (name "~{OE}")
          (number "13")
        )
        (pin input line (at -10.16 10.16 0) (length 2.54)
          (name "SER")
          (number "14")
        )
        (pin tri_state line (at 10.16 10.16 180) (length 2.54)
          (name "QA")
          (number "15")
        )
        (pin power_in line (at 0 15.24 270) (length 2.54)
          (name "VCC")
          (number "16")
        )
        (pin tri_state line (at 10.16 5.08 180) (length 2.54)
          (name "QC")
          (number "2")
        )
        (pin tri_state line (at 10.16 2.54 180) (length 2.54)
          (name "QD")
          (number "3")
        )
        (pin tri_state line (at 10.16 0 180) (length 2.54)
          (name "QE")
          (number "4")
        )
        (pin tri_state line (at 10.16 -2.54 180) (length 2.54)
          (name "QF")
          (number "5")
        )
        (pin tri_state line (at 10.16 -5.08 180) (length 2.54)
          (name "QG")
          (number "6")
        )
        (pin tri_state line (at 10.16 -7.62 180) (length 2.54)
          (name "QH")
          (number "7")
        )
        (pin power_in line (at 0 -17.78 90) (length 2.54)
          (name "GND")
          (number "8")
        )
        (pin output line (at 10.16 -12.7 180) (length 2.54)
          (name "QH'")
          (number "9")
        )
      )
      (symbol "74HC595_1_1"
        (rectangle (start -7.62 12.7) (end 7.62 -15.24)
          (fill (type background))
        )
      )
    )
    (symbol "Connector:AVR-ISP-6" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at -6.35 11.43 0))
      (property "Value" "AVR-ISP-6" (at 0 11.43 0))
      (property "Footprint" "" (at -6.35 1.27 90))
      (property "Datasheet" " ~" (at -32.385 -13.97 0))
      (property "ki_keywords" "AVR ISP Connector" (at 0 0 0))
      (property "ki_description" "Atmel 6-pin ISP connector" (at 0 0 0))
      (property "ki_fp_filters" "IDC?Header*2x03* Pin?Header*2x03*" (at 0 0 0))
      (symbol "AVR-ISP-6_0_1"
        (rectangle (start -2.667 -6.858) (end -2.413 -7.62)
          (fill (type none))
        )
        (rectangle (start -2.667 10.16) (end -2.413 9.398)
          (fill (type none))
        )
        (rectangle (start 7.62 -2.413) (end 6.858 -2.667)
          (fill (type none))
        )
        (rectangle (start 7.62 0.127) (end 6.858 -0.127)
          (fill (type none))
        )
        (rectangle (start 7.62 2.667) (end 6.858 2.413)
          (fill (type none))
        )
        (rectangle (start 7.62 5.207) (end 6.858 4.953)
          (fill (type none))
        )
        (rectangle (start 7.62 10.16) (end -7.62 -7.62)
          (fill (type background))
        )
      )
      (symbol "AVR-ISP-6_1_1"
        (pin passive line (at 10.16 5.08 180) (length 2.54)
          (name "MISO")
          (number "1")
        )
        (pin passive line (at -2.54 12.7 270) (length 2.54)
          (name "VCC")
          (number "2")
        )
        (pin passive line (at 10.16 0 180) (length 2.54)
          (name "SCK")
          (number "3")
        )
        (pin passive line (at 10.16 2.54 180) (length 2.54)
          (name "MOSI")
          (number "4")
        )
        (pin passive line (at 10.16 -2.54 180) (length 2.54)
          (name "~{RST}")
          (number "5")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "GND")
          (number "6")
        )
      )
    )
    (symbol "Device:Battery" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "BT" (at 2.54 2.54 0))
      (property "Value" "Battery" (at 2.54 0 0))
      (property "Footprint" "" (at 0 1.524 90))
      (property "Datasheet" "~" (at 0 1.524 90))
      (property "ki_keywords" "batt voltage-source cell" (at 0 0 0))
      (property "ki_description" "Multiple-cell battery" (at 0 0 0))
      (symbol "Battery_0_1"
        (rectangle (start -2.286 -1.27) (end 2.286 -1.524)
          (fill (type outline))
        )
        (rectangle (start -2.286 1.778) (end 2.286 1.524)
          (fill (type outline))
        )
        (rectangle (start -1.524 -2.032) (end 1.524 -2.54)
          (fill (type outline))
        )
        (rectangle (start -1.524 1.016) (end 1.524 0.508)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 -1.016)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.508)
            (xy 0 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.778)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 3.048)
            (xy 1.778 3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 3.556)
            (xy 1.27 2.54)
          )
          (fill (type none))
        )
      )
      (symbol "Battery_1_1"
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "-")
          (number "2")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "LED" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "LED diode" (at 0 0 0))
      (property "ki_description" "Light emitting diode" (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R_US" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.54 0 90))
      (property "Value" "R_US" (at -2.54 0 90))
      (property "Footprint" "" (at 1.016 -0.254 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor, US symbol" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_US_0_1"
        (polyline
          (pts
            (xy 0 -2.286)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.762)
            (xy 1.016 -1.143)
            (xy 0 -1.524)
            (xy -1.016 -1.905)
            (xy 0 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 1.016 0.381)
            (xy 0 0)
            (xy -1.016 -0.381)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 1.016 1.905)
            (xy 0 1.524)
            (xy -1.016 1.143)
            (xy 0 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "R_US_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Display_Character:Adafruit_7-segment_LED_HT16K33_Backpack" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -16.51 7.62 0))
      (property "Value" "" (at -24.13 15.24 0))
      (property "Footprint" "" (at -24.13 15.24 0))
      (property "Datasheet" "https://learn.adafruit.com/assets/108790" (at -24.13 15.24 0))
      (property "ki_keywords" "Adafruit 4-Digit 7-Segment LED I2C Backpack" (at 0 0 0))
      (property "ki_description" "Adafruit 0.56\" 4-Digit 7-Segment Display w/ I2C Backpack - STEMMA QT / qwiic" (at 0 0 0))
      (symbol "Adafruit_7-segment_LED_HT16K33_Backpack_0_1"
        (rectangle (start -3.81 -3.683) (end -3.81 -3.683)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 -3.683)
            (xy -3.81 -3.683)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -3.683)
            (xy 2.54 -3.683)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 8.89 -3.683)
            (xy 8.89 -3.683)
          )
          (fill (type none))
        )
        (rectangle (start 2.54 -3.683) (end 2.54 -3.683)
          (fill (type none))
        )
        (rectangle (start 8.89 -3.683) (end 8.89 -3.683)
          (fill (type none))
        )
      )
      (symbol "Adafruit_7-segment_LED_HT16K33_Backpack_1_0"
        (text "A" (at -7.366 2.54 0))
        (text "B" (at -5.08 1.778 0))
        (text "C" (at -5.334 -1.27 0))
        (text "D" (at -7.874 -2.032 0))
        (text "DP" (at -4.064 -2.794 0))
        (text "E" (at -10.16 -1.27 0))
        (text "F" (at -9.906 1.778 0))
        (text "G" (at -7.62 1.016 0))
        (text "L1" (at 2.032 2.286 0))
        (text "L2" (at 1.778 -1.778 0))
      )
      (symbol "Adafruit_7-segment_LED_HT16K33_Backpack_1_1"
        (rectangle (start -17.78 6.35) (end 19.05 -6.35)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -9.144 -0.254)
            (xy -9.398 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -8.89 -2.794)
            (xy -6.858 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -8.89 2.794)
            (xy -9.144 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -8.636 0.254)
            (xy -6.604 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -8.382 3.302)
            (xy -6.35 3.302)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.096 -0.254)
            (xy -6.35 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.842 2.794)
            (xy -6.096 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -2.921)
            (xy -5.08 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.794 -0.254)
            (xy -3.048 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.794)
            (xy -0.508 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.794)
            (xy -2.794 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.286 0.254)
            (xy -0.254 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 3.302)
            (xy 0 3.302)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 -0.254)
            (xy 0 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.508 2.794)
            (xy 0.254 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.921)
            (xy 1.27 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.778 -0.889)
            (xy 1.778 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.032 1.143)
            (xy 2.032 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.556 -0.254)
            (xy 3.302 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 -2.794)
            (xy 5.842 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 2.794)
            (xy 3.556 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.064 0.254)
            (xy 6.096 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 3.302)
            (xy 6.35 3.302)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 6.604 -0.254)
            (xy 6.35 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 6.858 2.794)
            (xy 6.604 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.62 -2.921)
            (xy 7.62 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 9.906 -0.254)
            (xy 9.652 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.16 -2.794)
            (xy 12.192 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.16 2.794)
            (xy 9.906 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.414 0.254)
            (xy 12.446 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.668 3.302)
            (xy 12.7 3.302)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 12.954 -0.254)
            (xy 12.7 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 13.208 2.794)
            (xy 12.954 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 13.97 -2.921)
            (xy 13.97 -2.794)
          )
          (fill (type none))
        )
        (text "Adafruit 7-segment\nLED HT16K33 Backpack" (at 19.05 8.89 0))
        (pin power_in line (at -20.32 1.27 0) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin input line (at -20.32 -3.81 0) (length 2.54)
          (name "SCL")
          (number "26")
        )
        (pin bidirectional line (at -20.32 -1.27 0) (length 2.54)
          (name "SDA")
          (number "27")
        )
        (pin power_in line (at -20.32 3.81 0) (length 2.54)
          (name "VDD")
          (number "28")
        )
      )
    )
    (symbol "MCU_Microchip_ATtiny:ATtiny84-20P" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -12.7 21.59 0))
      (property "Value" "ATtiny84-20P" (at 2.54 -21.59 0))
      (property "Footprint" "Package_DIP:DIP-14_W7.62mm" (at 0 0 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf" (at 0 0 0))
      (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR" (at 0 0 0))
      (property "ki_description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-14" (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (at 0 0 0))
      (symbol "ATtiny84-20P_0_1"
        (rectangle (start -12.7 -20.32) (end 12.7 20.32)
          (fill (type background))
        )
      )
      (symbol "ATtiny84-20P_1_1"
        (pin power_in line (at 0 22.86 270) (length 2.54)
          (name "VCC")
          (number "1")
        )
        (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
          (name "PA3")
          (number "10")
        )
        (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
          (name "PA2")
          (number "11")
        )
        (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
          (name "PA1")
          (number "12")
        )
        (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
          (name "AREF/PA0")
          (number "13")
        )
        (pin power_in line (at 0 -22.86 90) (length 2.54)
          (name "GND")
          (number "14")
        )
        (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
          (name "XTAL1/PB0")
          (number "2")
        )
        (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
          (name "XTAL2/PB1")
          (number "3")
        )
        (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
          (name "~{RESET}/PB3")
          (number "4")
        )
        (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
          (name "PB2")
          (number "5")
        )
        (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
          (name "PA7")
          (number "6")
        )
        (pin bidirectional line (at 15.24 0 180) (length 2.54)
          (name "PA6")
          (number "7")
        )
        (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
          (name "PA5")
          (number "8")
        )
        (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
          (name "PA4")
          (number "9")
        )
      )
    )
    (symbol "Regulator_Switching:Adafruit_MiniBoost_5V" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 3.81 6.35 0))
      (property "Value" "" (at 0 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "Adafruit MiniBoost 5V TPS61023" (at 0 0 0))
      (property "ki_description" "Adafruit MiniBoost 5V @ 1A - TPS61023" (at 0 0 0))
      (symbol "Adafruit_MiniBoost_5V_1_1"
        (rectangle (start -5.08 5.08) (end 5.08 -5.08)
          (fill (type background))
        )
        (text "Adafruit\nMiniBoost\nTPS61023" (at -8.89 -5.08 900))
        (pin power_in line (at -1.27 7.62 270) (length 2.54)
          (name "VIN")
          (number "1")
        )
        (pin power_in line (at -1.27 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin power_out line (at 7.62 2.54 180) (length 2.54)
          (name "5V")
          (number "3")
        )
        (pin input line (at 7.62 -2.54 180) (length 2.54)
          (name "EN")
          (number "4")
        )
      )
    )
    (symbol "Sensor_Magnetic:US5881LUA" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 5.08 6.35 0))
      (property "Value" "" (at 0 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "https://media.melexis.com/-/media/files/documents/datasheets/US5881-datasheet-melexis.pdf" (at 0 0 0))
      (property "ki_keywords" "Hall Effect Sensor Switch" (at 0 0 0))
      (property "ki_description" "Hall Effect Sensor Switch" (at 0 0 0))
      (symbol "US5881LUA_1_1"
        (rectangle (start -3.81 5.08) (end 6.35 -5.08)
          (fill (type background))
        )
        (text "US5881LUA" (at -5.08 -5.08 900))
        (pin power_in line (at 0 7.62 270) (length 2.54)
          (name "VDD")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin output line (at 8.89 0 180) (length 2.54)
          (name "OUT")
          (number "3")
        )
      )
    )
    (symbol "Switch:SW_DPST_x2" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (at 0 3.175 0))
      (property "Value" "SW_DPST_x2" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "switch lever" (at 0 0 0))
      (property "ki_description" "Single Pole Single Throw (SPST) switch, separate symbol" (at 0 0 0))
      (symbol "SW_DPST_x2_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.254)
            (xy 1.524 1.778)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "SW_DPST_x2_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B")
          (number "2")
        )
      )
      (symbol "SW_DPST_x2_2_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A")
          (number "3")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B")
          (number "4")
        )
      )
    )
    (symbol "Switch:SW_Push" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (at 1.27 2.54 0))
      (property "Value" "SW_Push" (at 0 -1.524 0))
      (property "Footprint" "" (at 0 5.08 0))
      (property "Datasheet" "~" (at 0 5.08 0))
      (property "ki_keywords" "switch normally-open pushbutton push-button" (at 0 0 0))
      (property "ki_description" "Push button switch, generic, two pins" (at 0 0 0))
      (symbol "SW_Push_0_1"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 170.815 43.18) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 152.4) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 118.11) (diameter 0) (color 0 0 0 0))
  (junction (at 36.83 166.37) (diameter 0) (color 0 0 0 0))
  (junction (at 21.59 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 170.815 18.415) (diameter 0) (color 0 0 0 0))
  (junction (at 21.59 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 140.97) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 175.26) (diameter 0) (color 0 0 0 0))
  (junction (at 21.59 27.94) (diameter 0) (color 0 0 0 0))
  (junction (at 146.685 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 144.145 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 20.32 143.51) (diameter 0) (color 0 0 0 0))
  (junction (at 21.59 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 20.32 132.08) (diameter 0) (color 0 0 0 0))
  (junction (at 36.83 177.8) (diameter 0) (color 0 0 0 0))
  (junction (at 167.005 111.76) (diameter 0) (color 0 0 0 0))
  (junction (at 36.83 154.94) (diameter 0) (color 0 0 0 0))
  (junction (at 20.32 120.65) (diameter 0) (color 0 0 0 0))
  (junction (at 36.83 189.23) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 163.83) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 36.83 120.65) (diameter 0) (color 0 0 0 0))
  (junction (at 149.225 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 36.83 132.08) (diameter 0) (color 0 0 0 0))
  (junction (at 36.83 109.22) (diameter 0) (color 0 0 0 0))
  (junction (at 36.83 143.51) (diameter 0) (color 0 0 0 0))
  (junction (at 182.245 28.575) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 20.32 109.22) (diameter 0) (color 0 0 0 0))
  (junction (at 20.32 154.94) (diameter 0) (color 0 0 0 0))
  (junction (at 167.005 66.04) (diameter 0) (color 0 0 0 0))
  (junction (at 21.59 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 21.59 48.26) (diameter 0) (color 0 0 0 0))
  (junction (at 20.32 166.37) (diameter 0) (color 0 0 0 0))
  (junction (at 20.32 177.8) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 67.31 189.23) (xy 36.83 189.23)))
  (wire (pts (xy 71.12 114.3) (xy 54.61 114.3)))
  (wire (pts (xy 69.85 38.1) (xy 52.07 38.1)))
  (wire (pts (xy 36.83 175.26) (xy 36.83 177.8)))
  (wire (pts (xy 64.77 124.46) (xy 64.77 177.8)))
  (wire (pts (xy 41.91 27.94) (xy 69.85 27.94)))
  (wire (pts (xy 151.765 83.82) (xy 144.145 83.82)))
  (wire (pts (xy 151.765 78.74) (xy 126.365 78.74)))
  (wire (pts (xy 57.15 143.51) (xy 36.83 143.51)))
  (wire (pts (xy 20.32 109.22) (xy 26.67 109.22)))
  (wire (pts (xy 36.83 118.11) (xy 36.83 120.65)))
  (wire (pts (xy 69.85 43.18) (xy 57.15 43.18)))
  (wire (pts (xy 71.12 121.92) (xy 62.23 121.92)))
  (wire (pts (xy 72.39 78.105) (xy 72.39 83.82)))
  (wire (pts (xy 20.32 109.22) (xy 20.32 120.65)))
  (wire (pts (xy 118.11 81.28) (xy 151.765 81.28)))
  (wire (pts (xy 142.24 18.415) (xy 151.765 18.415)))
  (wire (pts (xy 26.67 48.26) (xy 21.59 48.26)))
  (wire (pts (xy 20.32 154.94) (xy 26.67 154.94)))
  (wire (pts (xy 49.53 175.26) (xy 49.53 186.69)))
  (wire (pts (xy 151.765 86.36) (xy 149.225 86.36)))
  (wire (pts (xy 20.32 166.37) (xy 20.32 177.8)))
  (wire (pts (xy 21.59 68.58) (xy 21.59 78.74)))
  (wire (pts (xy 46.99 33.02) (xy 46.99 48.26)))
  (wire (pts (xy 182.245 28.575) (xy 184.15 28.575)))
  (wire (pts (xy 71.12 119.38) (xy 59.69 119.38)))
  (wire (pts (xy 151.765 88.9) (xy 146.685 88.9)))
  (wire (pts (xy 67.31 127) (xy 67.31 189.23)))
  (wire (pts (xy 44.45 30.48) (xy 44.45 38.1)))
  (wire (pts (xy 49.53 106.68) (xy 49.53 118.11)))
  (wire (pts (xy 151.765 99.06) (xy 133.985 99.06)))
  (wire (pts (xy 49.53 35.56) (xy 49.53 58.42)))
  (wire (pts (xy 49.53 152.4) (xy 49.53 163.83)))
  (wire (pts (xy 196.215 18.415) (xy 170.815 18.415)))
  (wire (pts (xy 44.45 106.68) (xy 49.53 106.68)))
  (wire (pts (xy 162.56 142.875) (xy 144.145 142.875)))
  (wire (pts (xy 190.5 81.915) (xy 190.5 111.76)))
  (wire (pts (xy 54.61 114.3) (xy 54.61 132.08)))
  (wire (pts (xy 36.83 152.4) (xy 36.83 154.94)))
  (wire (pts (xy 151.765 91.44) (xy 139.065 91.44)))
  (wire (pts (xy 44.45 129.54) (xy 49.53 129.54)))
  (polyline (pts (xy 136.525 57.785) (xy 198.12 57.785)))
  (wire (pts (xy 151.765 104.14) (xy 141.605 104.14)))
  (wire (pts (xy 146.685 88.9) (xy 133.985 88.9)))
  (wire (pts (xy 21.59 38.1) (xy 21.59 48.26)))
  (wire (pts (xy 133.985 86.36) (xy 69.85 86.36)))
  (wire (pts (xy 49.53 186.69) (xy 44.45 186.69)))
  (wire (pts (xy 59.69 154.94) (xy 36.83 154.94)))
  (wire (pts (xy 131.445 73.66) (xy 131.445 33.02)))
  (wire (pts (xy 21.59 78.74) (xy 21.59 88.9)))
  (wire (pts (xy 54.61 132.08) (xy 36.83 132.08)))
  (wire (pts (xy 136.525 114.3) (xy 88.9 114.3)))
  (wire (pts (xy 69.85 33.02) (xy 46.99 33.02)))
  (wire (pts (xy 144.145 83.82) (xy 144.145 142.875)))
  (wire (pts (xy 190.5 74.295) (xy 190.5 66.04)))
  (wire (pts (xy 52.07 38.1) (xy 52.07 68.58)))
  (wire (pts (xy 54.61 40.64) (xy 54.61 78.74)))
  (wire (pts (xy 71.12 116.84) (xy 57.15 116.84)))
  (wire (pts (xy 170.815 43.18) (xy 182.245 43.18)))
  (wire (pts (xy 57.15 43.18) (xy 57.15 88.9)))
  (wire (pts (xy 151.765 73.66) (xy 131.445 73.66)))
  (wire (pts (xy 36.83 109.22) (xy 71.12 109.22)))
  (wire (pts (xy 133.985 111.76) (xy 88.9 111.76)))
  (wire (pts (xy 128.905 76.2) (xy 128.905 27.94)))
  (wire (pts (xy 118.11 81.28) (xy 118.11 88.9)))
  (wire (pts (xy 59.69 119.38) (xy 59.69 154.94)))
  (wire (pts (xy 21.59 27.94) (xy 21.59 38.1)))
  (wire (pts (xy 149.225 86.36) (xy 136.525 86.36)))
  (wire (pts (xy 49.53 118.11) (xy 49.53 129.54)))
  (wire (pts (xy 131.445 109.22) (xy 88.9 109.22)))
  (wire (pts (xy 136.525 86.36) (xy 136.525 114.3)))
  (wire (pts (xy 44.45 140.97) (xy 49.53 140.97)))
  (wire (pts (xy 62.23 121.92) (xy 62.23 166.37)))
  (wire (pts (xy 69.85 86.36) (xy 69.85 75.565)))
  (wire (pts (xy 36.83 163.83) (xy 36.83 166.37)))
  (wire (pts (xy 146.685 140.335) (xy 146.685 88.9)))
  (wire (pts (xy 162.56 137.795) (xy 149.225 137.795)))
  (wire (pts (xy 139.065 91.44) (xy 139.065 127)))
  (wire (pts (xy 182.245 28.575) (xy 182.245 35.56)))
  (wire (pts (xy 142.24 36.83) (xy 142.24 38.735)))
  (wire (pts (xy 161.925 18.415) (xy 170.815 18.415)))
  (wire (pts (xy 44.45 152.4) (xy 49.53 152.4)))
  (wire (pts (xy 26.67 68.58) (xy 21.59 68.58)))
  (wire (pts (xy 162.56 140.335) (xy 146.685 140.335)))
  (wire (pts (xy 36.83 186.69) (xy 36.83 189.23)))
  (wire (pts (xy 196.215 130.175) (xy 196.215 18.415)))
  (wire (pts (xy 20.32 120.65) (xy 20.32 132.08)))
  (wire (pts (xy 71.12 111.76) (xy 52.07 111.76)))
  (wire (pts (xy 72.39 78.105) (xy 74.93 78.105)))
  (wire (pts (xy 26.67 27.94) (xy 21.59 27.94)))
  (wire (pts (xy 21.59 48.26) (xy 21.59 58.42)))
  (wire (pts (xy 69.85 35.56) (xy 49.53 35.56)))
  (wire (pts (xy 57.15 116.84) (xy 57.15 143.51)))
  (wire (pts (xy 54.61 78.74) (xy 41.91 78.74)))
  (wire (pts (xy 139.065 127) (xy 88.9 127)))
  (wire (pts (xy 21.59 88.9) (xy 26.67 88.9)))
  (wire (pts (xy 170.815 46.355) (xy 170.815 43.18)))
  (wire (pts (xy 69.85 30.48) (xy 44.45 30.48)))
  (wire (pts (xy 142.24 18.415) (xy 142.24 26.67)))
  (wire (pts (xy 126.365 78.74) (xy 126.365 40.64)))
  (wire (pts (xy 20.32 104.14) (xy 20.32 109.22)))
  (wire (pts (xy 20.32 189.23) (xy 26.67 189.23)))
  (wire (pts (xy 151.765 101.6) (xy 131.445 101.6)))
  (wire (pts (xy 20.32 120.65) (xy 26.67 120.65)))
  (wire (pts (xy 44.45 175.26) (xy 49.53 175.26)))
  (wire (pts (xy 36.83 106.68) (xy 36.83 109.22)))
  (wire (pts (xy 106.68 104.14) (xy 118.11 104.14)))
  (wire (pts (xy 44.45 118.11) (xy 49.53 118.11)))
  (wire (pts (xy 52.07 68.58) (xy 41.91 68.58)))
  (wire (pts (xy 26.67 58.42) (xy 21.59 58.42)))
  (wire (pts (xy 20.32 177.8) (xy 26.67 177.8)))
  (wire (pts (xy 36.83 129.54) (xy 36.83 132.08)))
  (wire (pts (xy 149.225 137.795) (xy 149.225 86.36)))
  (wire (pts (xy 127 96.52) (xy 151.765 96.52)))
  (wire (pts (xy 133.985 99.06) (xy 133.985 111.76)))
  (polyline (pts (xy 136.525 12.065) (xy 136.525 57.785)))
  (wire (pts (xy 52.07 120.65) (xy 36.83 120.65)))
  (wire (pts (xy 170.815 18.415) (xy 170.815 23.495)))
  (wire (pts (xy 71.12 127) (xy 67.31 127)))
  (wire (pts (xy 131.445 101.6) (xy 131.445 109.22)))
  (wire (pts (xy 69.85 40.64) (xy 54.61 40.64)))
  (wire (pts (xy 49.53 163.83) (xy 49.53 175.26)))
  (wire (pts (xy 62.23 166.37) (xy 36.83 166.37)))
  (wire (pts (xy 141.605 145.415) (xy 162.56 145.415)))
  (wire (pts (xy 52.07 111.76) (xy 52.07 120.65)))
  (wire (pts (xy 141.605 104.14) (xy 141.605 145.415)))
  (wire (pts (xy 44.45 163.83) (xy 49.53 163.83)))
  (wire (pts (xy 167.005 66.04) (xy 190.5 66.04)))
  (wire (pts (xy 26.67 38.1) (xy 21.59 38.1)))
  (wire (pts (xy 190.5 111.76) (xy 167.005 111.76)))
  (wire (pts (xy 49.53 104.14) (xy 49.53 106.68)))
  (wire (pts (xy 133.985 88.9) (xy 133.985 86.36)))
  (wire (pts (xy 131.445 33.02) (xy 90.17 33.02)))
  (wire (pts (xy 21.59 58.42) (xy 21.59 68.58)))
  (wire (pts (xy 46.99 48.26) (xy 41.91 48.26)))
  (wire (pts (xy 57.15 88.9) (xy 41.91 88.9)))
  (wire (pts (xy 20.32 143.51) (xy 20.32 154.94)))
  (wire (pts (xy 170.815 43.18) (xy 170.815 38.735)))
  (wire (pts (xy 179.705 28.575) (xy 182.245 28.575)))
  (wire (pts (xy 49.53 129.54) (xy 49.53 140.97)))
  (wire (pts (xy 20.32 177.8) (xy 20.32 189.23)))
  (wire (pts (xy 20.32 154.94) (xy 20.32 166.37)))
  (wire (pts (xy 126.365 40.64) (xy 90.17 40.64)))
  (wire (pts (xy 151.765 76.2) (xy 128.905 76.2)))
  (wire (pts (xy 36.83 140.97) (xy 36.83 143.51)))
  (wire (pts (xy 20.32 143.51) (xy 26.67 143.51)))
  (wire (pts (xy 175.26 130.175) (xy 196.215 130.175)))
  (wire (pts (xy 49.53 58.42) (xy 41.91 58.42)))
  (wire (pts (xy 44.45 38.1) (xy 41.91 38.1)))
  (wire (pts (xy 21.59 26.67) (xy 21.59 27.94)))
  (wire (pts (xy 128.905 27.94) (xy 90.17 27.94)))
  (wire (pts (xy 20.32 132.08) (xy 20.32 143.51)))
  (wire (pts (xy 69.85 75.565) (xy 74.93 75.565)))
  (wire (pts (xy 20.32 132.08) (xy 26.67 132.08)))
  (wire (pts (xy 64.77 177.8) (xy 36.83 177.8)))
  (wire (pts (xy 144.145 83.82) (xy 72.39 83.82)))
  (wire (pts (xy 26.67 78.74) (xy 21.59 78.74)))
  (wire (pts (xy 71.12 124.46) (xy 64.77 124.46)))
  (wire (pts (xy 49.53 140.97) (xy 49.53 152.4)))
  (wire (pts (xy 20.32 166.37) (xy 26.67 166.37)))
  (text "Power supply" (at 137.795 56.515 0))
  (symbol (lib_id "Device:C") (at 190.5 78.105 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C2" (at 187.325 76.835 0))
    (property "Value" "0.1µF" (at 187.325 79.375 0))
    (property "Footprint" "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (at 189.5348 81.915 0))
    (property "Datasheet" "~" (at 190.5 78.105 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "C2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 88.9 119.38 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR019" (at 85.09 119.38 0))
    (property "Value" "+5V" (at 92.075 119.38 90))
    (property "Footprint" "" (at 88.9 119.38 0))
    (property "Datasheet" "" (at 88.9 119.38 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR019") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 74.93 70.485 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR013" (at 78.74 70.485 0))
    (property "Value" "+5V" (at 71.12 70.485 90))
    (property "Footprint" "" (at 74.93 70.485 0))
    (property "Datasheet" "" (at 74.93 70.485 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR013") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 40.64 129.54 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R10" (at 40.64 123.19 90))
    (property "Value" "1M" (at 40.64 125.73 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 40.894 128.524 90))
    (property "Datasheet" "~" (at 40.64 129.54 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R10") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 30.48 27.94 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R1" (at 30.48 21.59 90))
    (property "Value" "2.4K" (at 30.48 24.13 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 30.226 26.924 90))
    (property "Datasheet" "~" (at 30.48 27.94 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 49.53 104.14 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR015" (at 49.53 97.79 0))
    (property "Value" "GND" (at 49.53 99.06 0))
    (property "Footprint" "" (at 49.53 104.14 0))
    (property "Datasheet" "" (at 49.53 104.14 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR015") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "74xx:74HC595") (at 80.01 38.1 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U2" (at 77.8159 20.32 0))
    (property "Value" "74HC595" (at 77.8159 22.86 0))
    (property "Footprint" "Package_DIP:DIP-16_W7.62mm" (at 80.01 38.1 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc595.pdf" (at 80.01 38.1 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "digi-roll"
        (path
          (reference "U2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 80.01 130.81 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR010" (at 80.01 137.16 0))
    (property "Value" "GND" (at 80.01 135.89 0))
    (property "Footprint" "" (at 80.01 130.81 0))
    (property "Datasheet" "" (at 80.01 130.81 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR010") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 40.64 186.69 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R15" (at 40.64 180.34 90))
    (property "Value" "1M" (at 40.64 182.88 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 40.894 185.674 90))
    (property "Datasheet" "~" (at 40.64 186.69 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R15") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 167.005 111.76 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR01" (at 167.005 118.11 0))
    (property "Value" "GND" (at 167.005 116.84 0))
    (property "Footprint" "" (at 167.005 111.76 0))
    (property "Datasheet" "" (at 167.005 111.76 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:Battery") (at 142.24 31.75 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "BT1" (at 146.05 29.9085 0))
    (property "Value" "Battery" (at 146.05 32.4485 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (at 142.24 30.226 90))
    (property "Datasheet" "~" (at 142.24 30.226 90))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "BT1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 90.17 35.56 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR018" (at 86.36 35.56 0))
    (property "Value" "+5V" (at 93.345 35.56 90))
    (property "Footprint" "" (at 90.17 35.56 0))
    (property "Datasheet" "" (at 90.17 35.56 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR018") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 30.48 78.74 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R6" (at 30.48 72.39 90))
    (property "Value" "2.4K" (at 30.48 74.93 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 30.226 77.724 90))
    (property "Datasheet" "~" (at 30.48 78.74 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 30.48 48.26 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R3" (at 30.48 41.91 90))
    (property "Value" "2.4K" (at 30.48 44.45 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 30.226 47.244 90))
    (property "Datasheet" "~" (at 30.48 48.26 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 38.1 38.1 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D2" (at 36.5125 31.75 0))
    (property "Value" "LED" (at 36.5125 34.29 0))
    (property "Footprint" "LED_THT:LED_D5.0mm" (at 38.1 38.1 0))
    (property "Datasheet" "~" (at 38.1 38.1 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "D2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Display_Character:Adafruit_7-segment_LED_HT16K33_Backpack") (at 95.25 74.295 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U4" (at 115.57 72.003 0))
    (property "Value" "~" (at 71.12 59.055 0))
    (property "Footprint" "Zane:Adafruit_7_seg" (at 71.12 59.055 0))
    (property "Datasheet" "https://learn.adafruit.com/assets/108790" (at 71.12 59.055 0))
    (pin "1")
    (pin "26")
    (pin "27")
    (pin "28")
    (instances
      (project "digi-roll"
        (path
          (reference "U4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 40.64 152.4 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R12" (at 40.64 146.05 90))
    (property "Value" "1M" (at 40.64 148.59 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 40.894 151.384 90))
    (property "Datasheet" "~" (at 40.64 152.4 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R12") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 40.64 175.26 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R14" (at 40.64 168.91 90))
    (property "Value" "1M" (at 40.64 171.45 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 40.894 174.244 90))
    (property "Datasheet" "~" (at 40.64 175.26 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R14") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 21.59 26.67 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR014" (at 21.59 20.32 0))
    (property "Value" "GND" (at 21.59 21.59 0))
    (property "Footprint" "" (at 21.59 26.67 0))
    (property "Datasheet" "" (at 21.59 26.67 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR014") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "4xxx:4532") (at 80.01 118.11 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U3" (at 76.2 105.41 0))
    (property "Value" "~" (at 77.47 120.65 0))
    (property "Footprint" "Package_DIP:DIP-16_W7.62mm" (at 77.47 120.65 0))
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4532b.pdf" (at 77.47 120.65 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "digi-roll"
        (path
          (reference "U3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 38.1 58.42 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "D4" (at 36.5125 52.07 0))
    (property "Value" "LED" (at 36.5125 54.61 0))
    (property "Footprint" "LED_THT:LED_D5.0mm" (at 38.1 58.42 0))
    (property "Datasheet" "~" (at 38.1 58.42 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "D4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 38.1 48.26 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D3" (at 36.5125 41.91 0))
    (property "Value" "LED" (at 36.5125 44.45 0))
    (property "Footprint" "LED_THT:LED_D5.0mm" (at 38.1 48.26 0))
    (property "Datasheet" "~" (at 38.1 48.26 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "D3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 30.48 58.42 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R4" (at 30.48 52.07 90))
    (property "Value" "2.4K" (at 30.48 54.61 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 30.226 57.404 90))
    (property "Datasheet" "~" (at 30.48 58.42 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 40.64 106.68 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R8" (at 40.64 100.33 90))
    (property "Value" "1M" (at 40.64 102.87 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 40.894 105.664 90))
    (property "Datasheet" "~" (at 40.64 106.68 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_Push") (at 31.75 120.65 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SW2" (at 31.75 114.3 0))
    (property "Value" "SW_MEC_5E" (at 31.75 113.03 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H5mm" (at 31.75 113.03 0))
    (property "Datasheet" "~" (at 31.75 115.57 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "SW2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 40.64 140.97 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R11" (at 40.64 134.62 90))
    (property "Value" "1M" (at 40.64 137.16 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 40.894 139.954 90))
    (property "Datasheet" "~" (at 40.64 140.97 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R11") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_Push") (at 31.75 177.8 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SW7" (at 31.75 171.45 0))
    (property "Value" "SW_MEC_5E" (at 31.75 170.18 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H5mm" (at 31.75 170.18 0))
    (property "Datasheet" "~" (at 31.75 172.72 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "SW7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 38.1 78.74 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D6" (at 36.5125 72.39 0))
    (property "Value" "LED" (at 36.5125 74.93 0))
    (property "Footprint" "LED_THT:LED_D5.0mm" (at 38.1 78.74 0))
    (property "Datasheet" "~" (at 38.1 78.74 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "D6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 40.64 163.83 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R13" (at 40.64 157.48 90))
    (property "Value" "1M" (at 40.64 160.02 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 40.894 162.814 90))
    (property "Datasheet" "~" (at 40.64 163.83 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R13") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 74.93 73.025 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR012" (at 68.58 73.025 0))
    (property "Value" "GND" (at 71.12 73.025 90))
    (property "Footprint" "" (at 74.93 73.025 0))
    (property "Datasheet" "" (at 74.93 73.025 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR012") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_Push") (at 31.75 143.51 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SW4" (at 31.75 137.16 0))
    (property "Value" "SW_MEC_5E" (at 31.75 135.89 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H5mm" (at 31.75 135.89 0))
    (property "Datasheet" "~" (at 31.75 138.43 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "SW4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:AVR-ISP-6") (at 172.72 142.875 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "J1" (at 182.245 140.335 0))
    (property "Value" "AVR-ISP-6" (at 182.245 142.875 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (at 179.07 141.605 90))
    (property "Datasheet" " ~" (at 205.105 156.845 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (instances
      (project "digi-roll"
        (path
          (reference "J1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Sensor_Magnetic:US5881LUA") (at 118.11 96.52 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U5" (at 123.19 90.17 0))
    (property "Value" "~" (at 118.11 96.52 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (at 118.11 96.52 0))
    (property "Datasheet" "https://media.melexis.com/-/media/files/documents/datasheets/US5881-datasheet-melexis.pdf" (at 118.11 96.52 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "digi-roll"
        (path
          (reference "U5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 175.26 153.035 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR020" (at 175.26 159.385 0))
    (property "Value" "GND" (at 175.26 158.115 0))
    (property "Footprint" "" (at 175.26 153.035 0))
    (property "Datasheet" "" (at 175.26 153.035 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR020") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_Push") (at 31.75 166.37 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SW6" (at 31.75 160.02 0))
    (property "Value" "SW_MEC_5E" (at 31.75 158.75 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H5mm" (at 31.75 158.75 0))
    (property "Datasheet" "~" (at 31.75 161.29 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "SW6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 106.68 104.14 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR07" (at 106.68 97.79 0))
    (property "Value" "GND" (at 106.68 99.695 0))
    (property "Footprint" "" (at 106.68 104.14 0))
    (property "Datasheet" "" (at 106.68 104.14 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR07") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 167.005 66.04 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR05" (at 167.005 69.85 0))
    (property "Value" "+5V" (at 167.005 60.96 0))
    (property "Footprint" "" (at 167.005 66.04 0))
    (property "Datasheet" "" (at 167.005 66.04 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 182.245 39.37 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C1" (at 185.42 38.1 0))
    (property "Value" "0.1µF" (at 185.42 40.64 0))
    (property "Footprint" "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (at 183.2102 43.18 0))
    (property "Datasheet" "~" (at 182.245 39.37 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "C1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 170.815 46.355 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR03" (at 170.815 52.705 0))
    (property "Value" "GND" (at 170.815 51.435 0))
    (property "Footprint" "" (at 170.815 46.355 0))
    (property "Datasheet" "" (at 170.815 46.355 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_Push") (at 31.75 189.23 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SW8" (at 31.75 182.88 0))
    (property "Value" "SW_MEC_5E" (at 31.75 181.61 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H5mm" (at 31.75 181.61 0))
    (property "Datasheet" "~" (at 31.75 184.15 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "SW8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_DPST_x2") (at 156.845 18.415 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SW9" (at 156.845 15.24 0))
    (property "Value" "SW_DPST_x2" (at 156.845 14.605 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (at 156.845 18.415 0))
    (property "Datasheet" "~" (at 156.845 18.415 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "digi-roll"
        (path
          (reference "SW9") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "MCU_Microchip_ATtiny:ATtiny84-20P") (at 167.005 88.9 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 180.975 87.63 0))
    (property "Value" "ATtiny84-20P" (at 180.975 90.17 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm" (at 167.005 88.9 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf" (at 167.005 88.9 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "digi-roll"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 38.1 88.9 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D7" (at 36.5125 82.55 0))
    (property "Value" "LED" (at 36.5125 85.09 0))
    (property "Footprint" "LED_THT:LED_D5.0mm" (at 38.1 88.9 0))
    (property "Datasheet" "~" (at 38.1 88.9 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "D7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 184.15 28.575 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR04" (at 180.34 28.575 0))
    (property "Value" "+5V" (at 187.96 28.575 90))
    (property "Footprint" "" (at 184.15 28.575 0))
    (property "Datasheet" "" (at 184.15 28.575 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 80.01 55.88 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR011" (at 80.01 62.23 0))
    (property "Value" "GND" (at 80.01 60.96 0))
    (property "Footprint" "" (at 80.01 55.88 0))
    (property "Datasheet" "" (at 80.01 55.88 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR011") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 30.48 88.9 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R7" (at 30.48 82.55 90))
    (property "Value" "2.4K" (at 30.48 85.09 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 30.226 87.884 90))
    (property "Datasheet" "~" (at 30.48 88.9 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Regulator_Switching:Adafruit_MiniBoost_5V") (at 172.085 31.115 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U6" (at 175.895 24.13 0))
    (property "Value" "~" (at 172.085 31.115 0))
    (property "Footprint" "Zane:Adafruit_Miniboost" (at 172.085 31.115 0))
    (property "Datasheet" "" (at 172.085 31.115 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "digi-roll"
        (path
          (reference "U6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 20.32 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR016" (at 20.32 107.95 0))
    (property "Value" "+5V" (at 20.32 99.06 0))
    (property "Footprint" "" (at 20.32 104.14 0))
    (property "Datasheet" "" (at 20.32 104.14 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR016") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_Push") (at 31.75 109.22 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SW1" (at 31.75 102.87 0))
    (property "Value" "SW_MEC_5E" (at 31.75 101.6 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H5mm" (at 31.75 101.6 0))
    (property "Datasheet" "~" (at 31.75 104.14 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "SW1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 90.17 43.18 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR017" (at 96.52 43.18 0))
    (property "Value" "GND" (at 93.98 43.18 90))
    (property "Footprint" "" (at 90.17 43.18 0))
    (property "Datasheet" "" (at 90.17 43.18 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR017") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 142.24 38.735 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR02" (at 142.24 45.085 0))
    (property "Value" "GND" (at 142.24 43.815 0))
    (property "Footprint" "" (at 142.24 38.735 0))
    (property "Datasheet" "" (at 142.24 38.735 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 40.64 118.11 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R9" (at 40.64 111.76 90))
    (property "Value" "1M" (at 40.64 114.3 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 40.894 117.094 90))
    (property "Datasheet" "~" (at 40.64 118.11 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R9") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 30.48 68.58 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R5" (at 30.48 62.23 90))
    (property "Value" "2.4K" (at 30.48 64.77 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 30.226 67.564 90))
    (property "Datasheet" "~" (at 30.48 68.58 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 80.01 22.86 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR09" (at 80.01 26.67 0))
    (property "Value" "+5V" (at 80.01 17.78 0))
    (property "Footprint" "" (at 80.01 22.86 0))
    (property "Datasheet" "" (at 80.01 22.86 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR09") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 38.1 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D5" (at 36.5125 62.23 0))
    (property "Value" "LED" (at 36.5125 64.77 0))
    (property "Footprint" "LED_THT:LED_D5.0mm" (at 38.1 68.58 0))
    (property "Datasheet" "~" (at 38.1 68.58 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "D5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 38.1 27.94 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D1" (at 36.5125 21.59 0))
    (property "Value" "LED" (at 36.5125 24.13 0))
    (property "Footprint" "LED_THT:LED_D5.0mm" (at 38.1 27.94 0))
    (property "Datasheet" "~" (at 38.1 27.94 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "D1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 30.48 38.1 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R2" (at 30.48 31.75 90))
    (property "Value" "2.4K" (at 30.48 34.29 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 30.226 37.084 90))
    (property "Datasheet" "~" (at 30.48 38.1 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "R2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_Push") (at 31.75 154.94 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SW5" (at 31.75 148.59 0))
    (property "Value" "SW_MEC_5E" (at 31.75 147.32 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H5mm" (at 31.75 147.32 0))
    (property "Datasheet" "~" (at 31.75 149.86 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "SW5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_Push") (at 31.75 132.08 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SW3" (at 31.75 125.73 0))
    (property "Value" "SW_MEC_5E" (at 31.75 124.46 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H5mm" (at 31.75 124.46 0))
    (property "Datasheet" "~" (at 31.75 127 0))
    (pin "1")
    (pin "2")
    (instances
      (project "digi-roll"
        (path
          (reference "SW3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 80.01 105.41 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR08" (at 80.01 109.22 0))
    (property "Value" "+5V" (at 80.01 100.33 0))
    (property "Footprint" "" (at 80.01 105.41 0))
    (property "Datasheet" "" (at 80.01 105.41 0))
    (pin "1")
    (instances
      (project "digi-roll"
        (path
          (reference "#PWR08") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
